time -- hour of day.

model -- EV model.

driving -- whether the owner is driving or not.

connected -- whether the EV is connected to the charger or not.

soc -- state-of-charge in kWh (how much energy is in the battery) at the **beginning** of the ‘time’.

charge\_need -- how much energy does the car **during** the ‘time’.

cadaster -- cadaster unit number